True/False

Seek delay is the time to move the read head to the desired track

True

Seek delay is the time needed by the disk to place the desired sector under the read head

False

Rotational delay is the time needed by the disk to place the desired sector under the read head

True

Rotational delay is the time to rotate the read head to reach the desired track

False

Multiple choice

What is the average latency for an Hard Disk Drive?

A Time to wait for the sector

B Time to wait for the data transfer

C Time to wait for the head movement

D Time to wait for the cylinder